Ascii output

Varicode

Data sync

Lowpass Filter

Downsample by 10

Lowpass Filter

VCO input