|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  | Shift register with 22x (8 or 16) bit cells |  |  |  |  |  |  |

+

<< 1